**SCHEDULE ‘B’**

**NAME OF WORK: Providing and Fixing Power Factor Improvement Plant K-Electric Connection for Water Supply Scheme of Various Villages of Dumlottee Kathore District Karachi Operation Maintenance**

**HEAD OF ACCOUNT. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item of work** | **Qty.** | **Rate** | **Unit** | **Amount** |

1. Providing and fixing Circuit breaker 800 anm TP setting 500-800 amp(XS-800NJ)

on prepared board as required. (FSI. No: 202 P.No: 31)

1.0 No @ Rs. 90,956/- P.No Rs. 90,956/-

1. Providing and fixing DP i/c change over switch 500 volts 600 amp. on prepared board.

(ESI. No: 202 P.No: 30)

1.0 No @ Rs.69,014/- P.No Rs. 69,014/-

1. Providing and laying (main or Sub main PVC in sulated & PVC sheeted with 4 Core copper conductor 600 / 1000 volts size 240 mm2 (ESI. No: 111 P.No: 13)

24.0 Meters @ Rs.16,294/- P. Meter Rs. 3,91,056/-

**Total Rs. 5,51,026/-**

**CONDITION**

1. **Any error and emission in the description quantity rate unit will be governed by the revenant schedule of rate estimate.**
2. **The rate quoted by the contractor will be inclusive of transportation charges upto site work.**
3. **No premium will be allowed Non schedule items.**
4. **No Separate carriage will be paid to contractor.**
5. **The premium should be inclusive of all the taxes i/c series i/c etc.**
6. **The contractor will not be allowed to withdraw their tender or ask to refund call deposit for the period from one month to three months.**

**Executive Engineer**

**(CONTRACTOR) Public Health Engineering**

**Division Karachi**